**CONSTRUCTION PRODUCTS REGULATION 2020
DECLARATION OF PERFORMANCE**

1. Unique identification code of the product-type: **M2M+**
2. Intended use or uses of the construction product, in accordance with applicable harmonised technical specification, as foreseen by the manufacturer**: Double External pedestrian panic/emergency door set for commercial premises (or similar) with fire and/or smoke compartmentation and/or escape routes**
3. Name, registered trade name or registered trade mark and contact address of the manufacturer as required: **Bradbury Security (Part of Bradbury Group Ltd) 6 Atkinsons way, Foxhills industrial estate, North Lincolnshire, DN15 8QJ**
4. System or systems of assessment and verification of constancy of performance of the construction product as set out in CPR, Annex V: **System 1 and 3**
5. Harmonised standard: **EN 14351-1:2006 + A2:2016; EN 16034:2014**
6. Notified body: **Efectis: CE – 1812-CPR-1729**
7. Declared performance:

|  |  |  |
| --- | --- | --- |
| **Essential Characteristics** | **Performance** | **Harmonised Technical Specification** |
| Water tightness – non-shielded (A) | NPD | EN 14351-1:2006+A2:2016 |
| Water tightness – shielded (B) | NPD |
| Dangerous substances | None |
| Resistance to wind load – test pressure | NPD |
| Resistance to wind load – frame deflection | NPD |
| Load bearing capacity of safety devices | NPD |
| Height | Up to 2454mm |
| Acoustic performance | Up to 35dB |
| Thermal transmittance | 3.4 W/m2K |
| Air permeability | NPD |
| Ability to release | EN 1125 and EN 179 |
| Resistance to fire (For fire compartmentation uses):  E: E1: E2: EW: | 90NPDNPDNPD | EN 16034:2014 |
| Smoke control | NPD |
| Self-closing | C |
| Durability of ability to release | NPD |
| Durability of self-closing:* Against degradation (cycle testing):
* Against ageing (corrosion):
 | NPDNPD |

The performance of the product identified above is in conformity with the declared performances. This declaration of performance is issued under the sole responsibility of the manufacturer identified in point 3. Signed for and on behalf of the manufacturer by:

**James Benson, Compliance manager**

